{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Bill of Materials","BoM_BAT","Data"],"not_rendered":{"charts":0,"images":11,"macros":1,"external_links":0,"defined_names":26,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Bill of Materials","index":0,"n_rows":6,"n_cols":8,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["xx",null,null,null,"Project Name:",null,null,"Name:"]
[{"$f":"NOW()","v":"2023-07-21T08:39:13.700"},null,null,null,null,null,null,"Address:"]
["Online Core Catalog ",null,null,null,null,null,null,"Phone Number:"]
["Download CN BOM Tool",null,null,null,null,null,null,"E-mail:"]
["zz",null,null,null,null,null,null,"Application:"]
["Description/Location","Part Number","Spec Sheet","Quantity","Total. Quantity","Comment"]

{"sheet":"BoM_BAT","index":1,"n_rows":255,"n_cols":13,"rows_kept":255,"cut":false,"hidden":true,"merged":[]}
[null,"Housing",null,"Short","Ultrashort",null,"Splice & Patch",null,null,null,"Connectivity Type","Connector"]
[null,"BATMGE","BAT-MGE-ST001","BAT (M) HOUSING - STD GREY EMKA","BATMGE",null,"FS","BAT-F-01","BAT Fusion Splice Module","FS","00"]
[null,"BATMGS","BAT-MGS-ST001","BAT (M) HOUSING - STD GREY SCREW","BATMGS",null,"RG","BAT-R-01","Routing Guide","RG"]
[null,"BATLGE","BAT-LGE-ST001","BAT (L) HOUSING - STD GREY EMKA","BATLGE",null,"PK","BAT-I-01","BAT Parking Module up to 16x SC Adapters","PK"]
[null,"BATLGS","BAT-LGS-ST001","BAT (L) HOUSING - STD GREY SCREW","BATLGS",null,"FA","BAT-CLT-01","BAT KIT - FANOUT FOR LT 3MM 10pcs SP","FA"]
[null,"BATXGE","BAT-XGE-ST001","BAT (XL) HOUSING - STD GREY EMKA","BATXGE",null,"SR","BAT-CCE-01","Internal Strain Relief","SR"]
[null,"BATXGS","BAT-XGS-ST001","BAT (XL) HOUSING - STD GREY SCREW","BATXGS",null,"BT","BAT-BTS-01","Buffer Tube Storage","BT"]
[null,"BATMGE","BAT-MWE-ST001","BAT (M) HOUSING - STD GREY EMKA","BATMGE",null,"xx",null,"Unused","xx"]
[null,"BATMGS","BAT-MGS-ST001","BAT (M) HOUSING - STD GREY SCREW","BATMGS",null,"05","Space 5mm","Space 5mm","05"]
[null,"BATLGE","BAT-LGE-ST001","BAT (L) HOUSING - STD GREY EMKA","BATLGE",null,20,"Space 20mm","Space 20mm",20]
[null,"BATLGS","BAT-LGS-ST001","BAT (L) HOUSING - STD GREY SCREW","BATLGS",null,50,"Space 50mm","Space 50mm",50]
[null,"BATXGE","BAT-XGE-ST001","BAT (XL) HOUSING - STD GREY EMKA","BATXGE",null,"2L","BAT-PTN-22RT","PM 2 ADPT LCA","2L","22","00"]
[null,"BATXGS","BAT-XGS-ST001","BAT (XL) HOUSING - STD GREY SCREW","BATXGS",null,"2M","BAT-PTY-22RT","PM 2 ADPT W/ PIGT LCA","2M","22","22"]
[null,null,"BAT-PLATE-M-01","BAT (M) METAL PLATE FOR STRAIN RELIEFS",null,null,"4L","BAT-PLN-22RT","PM 4 ADPT LCA","4L","22","00"]
[null,null,"BAT-PLATE-L-01","BAT (L) METAL PLATE FOR STRAIN RELIEFS",null,null,"4M","BAT-PLY-22RT","PM 4 ADPT W/ PIGT LCA","4M","22","22"]
[null,null,"BAT-PLATE-X-01","BAT (X) METAL PLATE FOR STRAIN RELIEFS",null,null,"2S","BAT-PTN-44RT","PM 2 ADPT SCA","2S","6C","00"]
[null,"BATMBE","BAT-MBE-ST001","BAT (M) HOUSING - STD BLACK EMKA",{"$f":"B17","v":"BATMBE"},null,"2T","BAT-PTY-44RT","PM 2 ADPT W/ PIGT SCA","2T","6C","44"]
[null,"BATMBS","BAT-MBS-ST001","BAT (M) HOUSING - STD BLACK SCREW","BATMBS",null,"4S","BAT-PLN-44RT","PM 4 ADPT SCA","4S","6C","00"]
[null,"BATLBE","BAT-LBE-ST001","BAT (L) HOUSING - STD BLACK EMKA","BATLBE",null,"4T","BAT-PLY-44RT","PM 4 ADPT W/ PIGT SCA","4T","6C","44"]
[null,"BATLBS","BAT-LBS-ST001","BAT (L) HOUSING - STD BLACK SCREW","BATLBS",null,"2N","BAT-PTN-02RT","BAT-P PM 2 ADPT, LCU","2N","02","00"]
[null,"BATXBE","BAT-XBE-ST001","BAT (XL) HOUSING - STD BLACK EMKA","BATXBE",null,"2O","BAT-PTY-02RT","BAT-P PM 2 ADPT W/ PIGT, LCU","2O","02","02"]
[null,"BATXBS","BAT-XBS-ST001","BAT (XL) HOUSING - STD BLACK SCREW","BATXBS",null,"4N","BAT-PLN-02RT","BAT-P PM 4 ADPT, LCU","4N","02","00"]
[null,null,null,null,null,null,"4O","BAT-PLY-02RT","BAT-P PM 4 ADPT W/ PIGT, LCU","4O","02","02"]
[null,null,null,null,null,null,"2U","BAT-PTN-58RT","BAT-P PM 2 ADPT, SCU","2U","5U","00"]
[null,null,null,null,null,null,"2V","BAT-PTY-58RT","BAT-P PM 2 ADPT W/ PIGT, SCU","2V","5U","58"]
[null,null,null,null,null,null,"4U","BAT-PLN-58RT","BAT-P PM 4 ADPT, SCU","4U","5U","00"]
[null,null,null,null,null,null,"4V","BAT-PLY-58RT","BAT-P PM 4 ADPT W/ PIGT, SCU","4V","5U","58"]
[null,null,null,null,null,null,"HS","BAT-PHD-LN-44RT","BAT (M-X) - HD PATCH MODULE 4 ADPT SCA","HS","6C"]
[null,null,null,null,null,null,"HT","BAT-PHD-LY-44RT","BAT (M-X) - HD PATCH MOD 4 ADPT W/ PIGT SCA","HT","6C"]
[null,null,null,null,null,null,"HU","BAT-PHD-LN-58RT","BAT (M-X) - HD PATCH MODULE 4 ADPT SCU","HU","5U"]
[null,null,null,null,null,null,"HV","BAT-PHD-LY-58RT","BAT (M-X) - HD PATCH MOD 4 ADPT W/ PIGT SCU","HV","5U"]
[null,null,null,null,null,null,"HL","BAT-PHD-LN-22RT","BAT (M-X) - HD PATCH MODULE 4 ADPT SCA","HL","6C"]
[null,null,null,null,null,null,"HM","BAT-PHD-LY-22RT","BAT (M-X) - HD PATCH MOD 4 ADPT W/ PIGT SCA","HM","6C"]
[null,null,null,null,null,null,"HN","BAT-PHD-LN-02RT","BAT (M-X) - HD PATCH MODULE 4 ADPT SCU","HN","5U"]
[null,null,null,null,null,null,"HO","BAT-PHD-LY-02RT","BAT (M-X) - HD PATCH MOD 4 ADPT W/ PIGT SCU","HO","5U"]
[]
[null,null,null,null,null,null,"Splitters",null,null,null,"Connectivity Type","Splitter Input 1f / 2f","Splitter Output"]
[null,null,null,null,null,null,"A1","BAT-K0000-102-1","1-1X2 SPLICE/SPLICE","A1","00","1","02"]
[null,null,null,null,null,null,"A2","BAT-K0000-102-2","2-1X2 SPLICE/SPLICE","A2","00","1","02"]
[null,null,null,null,null,null,"A3","BAT-K0000-102-3","3-1X2 SPLICE/SPLICE","A3","00","1","02"]
[null,null,null,null,null,null,"A4","BAT-K0000-102-4","4-1X2 SPLICE/SPLICE","A4","00","1","02"]
[null,null,null,null,null,null,"A5","BAT-K0022-102-1","1-1X2 SPLICE/LCAPC","A5","22","1","02"]
[null,null,null,null,null,null,"A6","BAT-K0022-102-2","2-1X2 SPLICE/LCAPC","A6","22","1","02"]
[null,null,null,null,null,null,"A7","BAT-K0022-102-3","3-1X2 SPLICE/LCAPC","A7","22","1","02"]
[null,null,null,null,null,null,"A8","BAT-K0022-102-4","4-1X2 SPLICE/LCAPC","A8","22","1","02"]
[null,null,null,null,null,null,"A9","BAT-K0044-102-1","1-1X2 SPLICE/SCAPC","A9","6C","1","02"]
[null,null,null,null,null,null,"A0","BAT-K0044-102-2","2-1X2 SPLICE/SCAPC","A0","6C","1","02"]
[null,null,null,null,null,null,"AA","BAT-K0044-102-3","3-1X2 SPLICE/SCAPC","AA","6C","1","02"]
[null,null,null,null,null,null,"AB","BAT-K0044-102-4","4-1X2 SPLICE/SCAPC","AB","6C","1","02"]
[null,null,null,null,null,null,"AC","BAT-K2200-102-1","1-1X2 LCAPC/SPLICE","AC","00","1","02"]
[null,null,null,null,null,null,"AD","BAT-K2200-102-2","2-1X2 LCAPC/SPLICE","AD","00","1","02"]
[null,null,null,null,null,null,"AE","BAT-K2200-102-3","3-1X2 LCAPC/SPLICE","AE","00","1","02"]
[null,null,null,null,null,null,"AF","BAT-K2200-102-4","4-1X2 LCAPC/SPLICE","AF","00","1","02"]
[null,null,null,null,null,null,"AG","BAT-K2222-102-1","1-1X2 LCAPC/LCAPC","AG","22","1","02"]
[null,null,null,null,null,null,"AH","BAT-K2222-102-2","2-1X2 LCAPC/LCAPC","AH","22","1","02"]
[null,null,null,null,null,null,"AI","BAT-K2222-102-3","3-1X2 LCAPC/LCAPC","AI","22","1","02"]
[null,null,null,null,null,null,"AJ","BAT-K2222-102-4","4-1X2 LCAPC/LCAPC","AJ","22","1","02"]
[null,null,null,null,null,null,"AK","BAT-K2244-102-1","1-1X2 LCAPC/SCAPC","AK","6C","1","02"]
[null,null,null,null,null,null,"AL","BAT-K2244-102-2","2-1X2 LCAPC/SCAPC","AL","6C","1","02"]
[null,null,null,null,null,null,"AM","BAT-K2244-102-3","3-1X2 LCAPC/SCAPC","AM","6C","1","02"]
[null,null,null,null,null,null,"AN","BAT-K2244-102-4","4-1X2 LCAPC/SCAPC","AN","6C","1","02"]
[null,null,null,null,null,null,"AO","BAT-K4400-102-1","1-1X2 SCAPC/SPLICE","AO","00","1","02"]
[null,null,null,null,null,null,"AP","BAT-K4400-102-2","2-1X2 SCAPC/SPLICE","AP","00","1","02"]
[null,null,null,null,null,null,"AQ","BAT-K4400-102-3","3-1X2 SCAPC/SPLICE","AQ","00","1","02"]
[null,null,null,null,null,null,"AR","BAT-K4400-102-4","4-1X2 SCAPC/SPLICE","AR","00","1","02"]
[null,null,null,null,null,null,"AS","BAT-K4422-102-1","1-1X2 SCAPC/LCAPC","AS","22","1","02"]
[null,null,null,null,null,null,"AT","BAT-K4422-102-2","2-1X2 SCAPC/LCAPC","AT","22","1","02"]
[null,null,null,null,null,null,"AU","BAT-K4422-102-3","3-1X2 SCAPC/LCAPC","AU","22","1","02"]
[null,null,null,null,null,null,"AV","BAT-K4422-102-4","4-1X2 SCAPC/LCAPC","AV","22","1","02"]
[null,null,null,null,null,null,"AW","BAT-K4444-102-1","1-1X2 SCAPC/SCAPC","AW","6C","1","02"]
[null,null,null,null,null,null,"AX","BAT-K4444-102-2","2-1X2 SCAPC/SCAPC","AX","6C","1","02"]
[null,null,null,null,null,null,"AY","BAT-K4444-102-3","3-1X2 SCAPC/SCAPC","AY","6C","1","02"]
[null,null,null,null,null,null,"AZ","BAT-K4444-102-4","4-1X2 SCAPC/SCAPC","AZ","6C","1","02"]
[null,null,null,null,null,null,"B1","BAT-K0000-104-1","1-1X4 SPLICE/SPLICE","B1","00","1","04"]
[null,null,null,null,null,null,"B2","BAT-K0000-104-2","2-1X4 SPLICE/SPLICE","B2","00","1","04"]
[null,null,null,null,null,null,"B3","BAT-K0000-104-3","3-1X4 SPLICE/SPLICE","B3","00","1","04"]
[null,null,null,null,null,null,"B4","BAT-K0000-104-4","4-1X4 SPLICE/SPLICE","B4","00","1","04"]
[null,null,null,null,null,null,"B5","BAT-K0022-104-1","1-1X4 SPLICE/LCAPC","B5","22","1","04"]
[null,null,null,null,null,null,"B6","BAT-K0022-104-2","2-1X4 SPLICE/LCAPC","B6","22","1","04"]
[null,null,null,null,null,null,"B7","BAT-K0022-104-3","3-1X4 SPLICE/LCAPC","B7","22","1","04"]
[null,null,null,null,null,null,"B8","BAT-K0022-104-4","4-1X4 SPLICE/LCAPC","B8","22","1","04"]
[null,null,null,null,null,null,"B9","BAT-K0044-104-1","1-1X4 SPLICE/SCAPC","B9","6C","1","04"]
[null,null,null,null,null,null,"B0","BAT-K0044-104-2","2-1X4 SPLICE/SCAPC","B0","6C","1","04"]
[null,null,null,null,null,null,"BA","BAT-K0044-104-3","3-1X4 SPLICE/SCAPC","BA","6C","1","04"]
[null,null,null,null,null,null,"BB","BAT-K0044-104-4","4-1X4 SPLICE/SCAPC","BB","6C","1","04"]
[null,null,null,null,null,null,"BC","BAT-K2200-104-1","1-1X4 LCAPC/SPLICE","BC","00","1","04"]
[null,null,null,null,null,null,"BD","BAT-K2200-104-2","2-1X4 LCAPC/SPLICE","BD","00","1","04"]
[null,null,null,null,null,null,"BE","BAT-K2200-104-3","3-1X4 LCAPC/SPLICE","BE","00","1","04"]
[null,null,null,null,null,null,"BF","BAT-K2200-104-4","4-1X4 LCAPC/SPLICE","BF","00","1","04"]
[null,null,null,null,null,null,"BG","BAT-K2222-104-1","1-1X4 LCAPC/LCAPC","BG","22","1","04"]
[null,null,null,null,null,null,"BH","BAT-K2222-104-2","2-1X4 LCAPC/LCAPC","BH","22","1","04"]
[null,null,null,null,null,null,"BI","BAT-K2222-104-3","3-1X4 LCAPC/LCAPC","BI","22","1","04"]
[null,null,null,null,null,null,"BJ","BAT-K2222-104-4","4-1X4 LCAPC/LCAPC","BJ","22","1","04"]
[null,null,null,null,null,null,"BK","BAT-K2244-104-1","1-1X4 LCAPC/SCAPC","BK","6C","1","04"]
[null,null,null,null,null,null,"BL","BAT-K2244-104-2","2-1X4 LCAPC/SCAPC","BL","6C","1","04"]
[null,null,null,null,null,null,"BM","BAT-K2244-104-3","3-1X4 LCAPC/SCAPC","BM","6C","1","04"]
[null,null,null,null,null,null,"BN","BAT-K2244-104-4","4-1X4 LCAPC/SCAPC","BN","6C","1","04"]
[null,null,null,null,null,null,"BO","BAT-K4400-104-1","1-1X4 SCAPC/SPLICE","BO","00","1","04"]
[null,null,null,null,null,null,"BP","BAT-K4400-104-2","2-1X4 SCAPC/SPLICE","BP","00","1","04"]
[null,null,null,null,null,null,"BQ","BAT-K4400-104-3","3-1X4 SCAPC/SPLICE","BQ","00","1","04"]
[null,null,null,null,null,null,"BR","BAT-K4400-104-4","4-1X4 SCAPC/SPLICE","BR","00","1","04"]
[null,null,null,null,null,null,"BS","BAT-K4422-104-1","1-1X4 SCAPC/LCAPC","BS","22","1","04"]
[null,null,null,null,null,null,"BT","BAT-K4422-104-2","2-1X4 SCAPC/LCAPC","BT","22","1","04"]
[null,null,null,null,null,null,"BU","BAT-K4422-104-3","3-1X4 SCAPC/LCAPC","BU","22","1","04"]
[null,null,null,null,null,null,"BV","BAT-K4422-104-4","4-1X4 SCAPC/LCAPC","BV","22","1","04"]
[null,null,null,null,null,null,"BW","BAT-K4444-104-1","1-1X4 SCAPC/SCAPC","BW","6C","1","04"]
[null,null,null,null,null,null,"BX","BAT-K4444-104-2","2-1X4 SCAPC/SCAPC","BX","6C","1","04"]
[null,null,null,null,null,null,"BY","BAT-K4444-104-3","3-1X4 SCAPC/SCAPC","BY","6C","1","04"]
[null,null,null,null,null,null,"BZ","BAT-K4444-104-4","4-1X4 SCAPC/SCAPC","BZ","6C","1","04"]
[null,null,null,null,null,null,"C1","BAT-K0000-108-1","1-1X8 SPLICE/SPLICE","C1","00","1","08"]
[null,null,null,null,null,null,"C2","BAT-K0000-108-2","2-1X8 SPLICE/SPLICE","C2","00","1","08"]
[null,null,null,null,null,null,"C3","BAT-K0000-108-3","3-1X8 SPLICE/SPLICE","C3","00","1","08"]
[null,null,null,null,null,null,"C4","BAT-K0000-108-4","4-1X8 SPLICE/SPLICE","C4","00","1","08"]
[null,null,null,null,null,null,"C5","BAT-K0022-108-1","1-1X8 SPLICE/LCAPC","C5","22","1","08"]
[null,null,null,null,null,null,"C6","BAT-K0022-108-2","2-1X8 SPLICE/LCAPC","C6","22","1","08"]
[null,null,null,null,null,null,"C7","BAT-K0022-108-3","3-1X8 SPLICE/LCAPC","C7","22","1","08"]
[null,null,null,null,null,null,"C8","BAT-K0022-108-4","4-1X8 SPLICE/LCAPC","C8","22","1","08"]
[null,null,null,null,null,null,"C9","BAT-K0044-108-1","1-1X8 SPLICE/SCAPC","C9","6C","1","08"]
[null,null,null,null,null,null,"C0","BAT-K0044-108-2","2-1X8 SPLICE/SCAPC","C0","6C","1","08"]
[null,null,null,null,null,null,"CA","BAT-K0044-108-3","3-1X8 SPLICE/SCAPC","CA","6C","1","08"]
[null,null,null,null,null,null,"CB","BAT-K0044-108-4","4-1X8 SPLICE/SCAPC","CB","6C","1","08"]
[null,null,null,null,null,null,"CC","BAT-K2200-108-1","1-1X8 LCAPC/SPLICE","CC","00","1","08"]
[null,null,null,null,null,null,"CD","BAT-K2200-108-2","2-1X8 LCAPC/SPLICE","CD","00","1","08"]
[null,null,null,null,null,null,"CE","BAT-K2200-108-3","3-1X8 LCAPC/SPLICE","CE","00","1","08"]
[null,null,null,null,null,null,"CF","BAT-K2200-108-4","4-1X8 LCAPC/SPLICE","CF","00","1","08"]
[null,null,null,null,null,null,"CG","BAT-K2222-108-1","1-1X8 LCAPC/LCAPC","CG","22","1","08"]
[null,null,null,null,null,null,"CH","BAT-K2222-108-2","2-1X8 LCAPC/LCAPC","CH","22","1","08"]
[null,null,null,null,null,null,"CI","BAT-K2222-108-3","3-1X8 LCAPC/LCAPC","CI","22","1","08"]
[null,null,null,null,null,null,"CJ","BAT-K2222-108-4","4-1X8 LCAPC/LCAPC","CJ","22","1","08"]
[null,null,null,null,null,null,"CK","BAT-K2244-108-1","1-1X8 LCAPC/SCAPC","CK","6C","1","08"]
[null,null,null,null,null,null,"CL","BAT-K2244-108-2","2-1X8 LCAPC/SCAPC","CL","6C","1","08"]
[null,null,null,null,null,null,"CM","BAT-K2244-108-3","3-1X8 LCAPC/SCAPC","CM","6C","1","08"]
[null,null,null,null,null,null,"CN","BAT-K2244-108-4","4-1X8 LCAPC/SCAPC","CN","6C","1","08"]
[null,null,null,null,null,null,"CO","BAT-K4400-108-1","1-1X8 SCAPC/SPLICE","CO","00","1","08"]
[null,null,null,null,null,null,"CP","BAT-K4400-108-2","2-1X8 SCAPC/SPLICE","CP","00","1","08"]
[null,null,null,null,null,null,"CQ","BAT-K4400-108-3","3-1X8 SCAPC/SPLICE","CQ","00","1","08"]
[null,null,null,null,null,null,"CR","BAT-K4400-108-4","4-1X8 SCAPC/SPLICE","CR","00","1","08"]
[null,null,null,null,null,null,"CS","BAT-K4422-108-1","1-1X8 SCAPC/LCAPC","CS","22","1","08"]
[null,null,null,null,null,null,"CT","BAT-K4422-108-2","2-1X8 SCAPC/LCAPC","CT","22","1","08"]
[null,null,null,null,null,null,"CU","BAT-K4422-108-3","3-1X8 SCAPC/LCAPC","CU","22","1","08"]
[null,null,null,null,null,null,"CV","BAT-K4422-108-4","4-1X8 SCAPC/LCAPC","CV","22","1","08"]
[null,null,null,null,null,null,"CW","BAT-K4444-108-1","1-1X8 SCAPC/SCAPC","CW","6C","1","08"]
[null,null,null,null,null,null,"CX","BAT-K4444-108-2","2-1X8 SCAPC/SCAPC","CX","6C","1","08"]
[null,null,null,null,null,null,"CY","BAT-K4444-108-3","3-1X8 SCAPC/SCAPC","CY","6C","1","08"]
[null,null,null,null,null,null,"CZ","BAT-K4444-108-4","4-1X8 SCAPC/SCAPC","CZ","6C","1","08"]
[null,null,null,null,null,null,"D1","BAT-K0000-116-1","1-1X16 SPLICE/SPLICE","D1","00","1","16"]
[null,null,null,null,null,null,"D2","BAT-K0022-116-1","1-1X16 SPLICE/LCAPC","D2","22","1","16"]
[null,null,null,null,null,null,"D3","BAT-K0044-116-1","1-1X16 SPLICE/SCAPC","D3","6C","1","16"]
[null,null,null,null,null,null,"D4","BAT-K2200-116-1","1-1X16 LCAPC/SPLICE","D4","00","1","16"]
[null,null,null,null,null,null,"D5","BAT-K2222-116-1","1-1X16 LCAPC/LCAPC","D5","22","1","16"]
[null,null,null,null,null,null,"D6","BAT-K2244-116-1","1-1X16 LCAPC/SCAPC","D6","6C","1","16"]
[null,null,null,null,null,null,"D7","BAT-K4400-116-1","1-1X16 SCAPC/SPLICE","D7","00","1","16"]
[null,null,null,null,null,null,"D8","BAT-K4422-116-1","1-1X16 SCAPC/LCAPC","D8","22","1","16"]
[null,null,null,null,null,null,"D9","BAT-K4444-116-1","1-1X16 SCAPC/SCAPC","D9","6C","1","16"]
[null,null,null,null,null,null,"E1","BAT-K0000-132-1","1-1X32 SPLICE/SPLICE","E1","00","1","32"]
[null,null,null,null,null,null,"E2","BAT-K0022-132-1","1-1X32 SPLICE/LCAPC","E2","22","1","32"]
[null,null,null,null,null,null,"E3","BAT-K0044-132-1","1-1X32 SPLICE/SCAPC","E3","6C","1","32"]
[null,null,null,null,null,null,"E4","BAT-K2200-132-1","1-1X32 LCAPC/SPLICE","E4","00","1","32"]
[null,null,null,null,null,null,"E5","BAT-K2222-132-1","1-1X32 LCAPC/LCAPC","E5","22","1","32"]
[null,null,null,null,null,null,"E6","BAT-K2244-132-1","1-1X32 LCAPC/SCAPC","E6","6C","1","32"]
[null,null,null,null,null,null,"E7","BAT-K4400-132-1","1-1X32 SCAPC/SPLICE","E7","00","1","32"]
[null,null,null,null,null,null,"E8","BAT-K4422-132-1","1-1X32 SCAPC/LCAPC","E8","22","1","32"]
[null,null,null,null,null,null,"E9","BAT-K4444-132-1","1-1X32 SCAPC/SCAPC","E9","6C","1","32"]
[null,null,null,null,null,null,"F1","BAT-K4444-164-1","1-1X64 SCAPC/SCAPC","F1","6C","1","64"]
[null,null,null,null,null,null,"F2","BAT-K0044-164-1","1-1X64 SPLICE/SCAPC","F2","6C","1","64"]
[null,null,null,null,null,null,"F3","BAT-K0022-164-1","1-1X64 SPLICE/LCAPC","F3",22,"1","64"]
[null,null,null,null,null,null,"F4","BAT-K2222-164-1","1-1X64 LCAPC/LCAPC","F4",22,"1","64"]
[null,null,null,null,null,null,"F5","BAT-K0000-164-1","1-1X64 SPLICE/SPLICE","F5",22,"1","64"]
[null,null,null,null,null,null,"G1","BAT-K0000-204-1","1-2X4 SPLICE/SPLICE","G1","00","2","04"]
[null,null,null,null,null,null,"G2","BAT-K0000-204-2","2-2X4 SPLICE/SPLICE","G2","00","2","04"]
[null,null,null,null,null,null,"G3","BAT-K0000-204-3","3-2X4 SPLICE/SPLICE","G3","00","2","04"]
[null,null,null,null,null,null,"G4","BAT-K0000-204-4","4-2X4 SPLICE/SPLICE","G4","00","2","04"]
[null,null,null,null,null,null,"G5","BAT-K0022-204-1","1-2X4 SPLICE/LCAPC","G5","22","2","04"]
[null,null,null,null,null,null,"G6","BAT-K0022-204-2","2-2X4 SPLICE/LCAPC","G6","22","2","04"]
[null,null,null,null,null,null,"G7","BAT-K0022-204-3","3-2X4 SPLICE/LCAPC","G7","22","2","04"]
[null,null,null,null,null,null,"G8","BAT-K0022-204-4","4-2X4 SPLICE/LCAPC","G8","22","2","04"]
[null,null,null,null,null,null,"G9","BAT-K0044-204-1","1-2X4 SPLICE/SCAPC","G9","6C","2","04"]
[null,null,null,null,null,null,"G0","BAT-K0044-204-2","2-2X4 SPLICE/SCAPC","G0","6C","2","04"]
[null,null,null,null,null,null,"GA","BAT-K0044-204-3","3-2X4 SPLICE/SCAPC","GA","6C","2","04"]
[null,null,null,null,null,null,"GB","BAT-K0044-204-4","4-2X4 SPLICE/SCAPC","GB","6C","2","04"]
[null,null,null,null,null,null,"GC","BAT-K2200-204-1","1-2X4 LCAPC/SPLICE","GC","00","2","04"]
[null,null,null,null,null,null,"GD","BAT-K2200-204-2","2-2X4 LCAPC/SPLICE","GD","00","2","04"]
[null,null,null,null,null,null,"GE","BAT-K2200-204-3","3-2X4 LCAPC/SPLICE","GE","00","2","04"]
[null,null,null,null,null,null,"GF","BAT-K2200-204-4","4-2X4 LCAPC/SPLICE","GF","00","2","04"]
[null,null,null,null,null,null,"GG","BAT-K2222-204-1","1-2X4 LCAPC/LCAPC","GG","22","2","04"]
[null,null,null,null,null,null,"GH","BAT-K2222-204-2","2-2X4 LCAPC/LCAPC","GH","22","2","04"]
[null,null,null,null,null,null,"GI","BAT-K2222-204-3","3-2X4 LCAPC/LCAPC","GI","22","2","04"]
[null,null,null,null,null,null,"GJ","BAT-K2222-204-4","4-2X4 LCAPC/LCAPC","GJ","22","2","04"]
[null,null,null,null,null,null,"GK","BAT-K2244-204-1","1-2X4 LCAPC/SCAPC","GK","6C","2","04"]
[null,null,null,null,null,null,"GL","BAT-K2244-204-2","2-2X4 LCAPC/SCAPC","GL","6C","2","04"]
[null,null,null,null,null,null,"GM","BAT-K2244-204-3","3-2X4 LCAPC/SCAPC","GM","6C","2","04"]
[null,null,null,null,null,null,"GN","BAT-K2244-204-4","4-2X4 LCAPC/SCAPC","GN","6C","2","04"]
[null,null,null,null,null,null,"GO","BAT-K4400-204-1","1-2X4 SCAPC/SPLICE","GO","00","2","04"]
[null,null,null,null,null,null,"GP","BAT-K4400-204-2","2-2X4 SCAPC/SPLICE","GP","00","2","04"]
[null,null,null,null,null,null,"GQ","BAT-K4400-204-3","3-2X4 SCAPC/SPLICE","GQ","00","2","04"]
[null,null,null,null,null,null,"GR","BAT-K4400-204-4","4-2X4 SCAPC/SPLICE","GR","00","2","04"]
[null,null,null,null,null,null,"GS","BAT-K4422-204-1","1-2X4 SCAPC/LCAPC","GS","22","2","04"]
[null,null,null,null,null,null,"GT","BAT-K4422-204-2","2-2X4 SCAPC/LCAPC","GT","22","2","04"]
[null,null,null,null,null,null,"GU","BAT-K4422-204-3","3-2X4 SCAPC/LCAPC","GU","22","2","04"]
[null,null,null,null,null,null,"GV","BAT-K4422-204-4","4-2X4 SCAPC/LCAPC","GV","22","2","04"]
[null,null,null,null,null,null,"GW","BAT-K4444-204-1","1-2X4 SCAPC/SCAPC","GW","6C","2","04"]
[null,null,null,null,null,null,"GX","BAT-K4444-204-2","2-2X4 SCAPC/SCAPC","GX","6C","2","04"]
[null,null,null,null,null,null,"GY","BAT-K4444-204-3","3-2X4 SCAPC/SCAPC","GY","6C","2","04"]
[null,null,null,null,null,null,"GZ","BAT-K4444-204-4","4-2X4 SCAPC/SCAPC","GZ","6C","2","04"]
[null,null,null,null,null,null,"H1","BAT-K0000-208-1","1-2X8 SPLICE/SPLICE","H1","00","2","08"]
[null,null,null,null,null,null,"H2","BAT-K0000-208-2","2-2X8 SPLICE/SPLICE","H2","00","2","08"]
[null,null,null,null,null,null,"H3","BAT-K0000-208-3","3-2X8 SPLICE/SPLICE","H3","00","2","08"]
[null,null,null,null,null,null,"H4","BAT-K0000-208-4","4-2X8 SPLICE/SPLICE","H4","00","2","08"]
[null,null,null,null,null,null,"H5","BAT-K0022-208-1","1-2X8 SPLICE/LCAPC","H5","22","2","08"]
[null,null,null,null,null,null,"H6","BAT-K0022-208-2","2-2X8 SPLICE/LCAPC","H6","22","2","08"]
[null,null,null,null,null,null,"H7","BAT-K0022-208-3","3-2X8 SPLICE/LCAPC","H7","22","2","08"]
[null,null,null,null,null,null,"H8","BAT-K0022-208-4","4-2X8 SPLICE/LCAPC","H8","22","2","08"]
[null,null,null,null,null,null,"H9","BAT-K0044-208-1","1-2X8 SPLICE/SCAPC","H9","6C","2","08"]
[null,null,null,null,null,null,"H0","BAT-K0044-208-2","2-2X8 SPLICE/SCAPC","H0","6C","2","08"]
[null,null,null,null,null,null,"HA","BAT-K0044-208-3","3-2X8 SPLICE/SCAPC","HA","6C","2","08"]
[null,null,null,null,null,null,"HB","BAT-K0044-208-4","4-2X8 SPLICE/SCAPC","HB","6C","2","08"]
[null,null,null,null,null,null,"HC","BAT-K2200-208-1","1-2X8 LCAPC/SPLICE","HC","00","2","08"]
[null,null,null,null,null,null,"HD","BAT-K2200-208-2","2-2X8 LCAPC/SPLICE","HD","00","2","08"]
[null,null,null,null,null,null,"HE","BAT-K2200-208-3","3-2X8 LCAPC/SPLICE","HE","00","2","08"]
[null,null,null,null,null,null,"HF","BAT-K2200-208-4","4-2X8 LCAPC/SPLICE","HF","00","2","08"]
[null,null,null,null,null,null,"HG","BAT-K2222-208-1","1-2X8 LCAPC/LCAPC","HG","22","2","08"]
[null,null,null,null,null,null,"HH","BAT-K2222-208-2","2-2X8 LCAPC/LCAPC","HH","22","2","08"]
[null,null,null,null,null,null,"HI","BAT-K2222-208-3","3-2X8 LCAPC/LCAPC","HI","22","2","08"]
[null,null,null,null,null,null,"HJ","BAT-K2222-208-4","4-2X8 LCAPC/LCAPC","HJ","22","2","08"]
[null,null,null,null,null,null,"HK","BAT-K2244-208-1","1-2X8 LCAPC/SCAPC","HK","6C","2","08"]
[null,null,null,null,null,null,"HP","BAT-K4400-208-2","2-2X8 SCAPC/SPLICE","HP","00","2","08"]
[null,null,null,null,null,null,"HQ","BAT-K4400-208-3","3-2X8 SCAPC/SPLICE","HQ","00","2","08"]
[null,null,null,null,null,null,"HR","BAT-K4400-208-4","4-2X8 SCAPC/SPLICE","HR","00","2","08"]
[null,null,null,null,null,null,"HW","BAT-K4444-208-1","1-2X8 SCAPC/SCAPC","HW","6C","2","08"]
[null,null,null,null,null,null,"HX","BAT-K4444-208-2","2-2X8 SCAPC/SCAPC","HX","6C","2","08"]
[null,null,null,null,null,null,"HY","BAT-K4444-208-3","3-2X8 SCAPC/SCAPC","HY","6C","2","08"]
[null,null,null,null,null,null,"HZ","BAT-K4444-208-4","4-2X8 SCAPC/SCAPC","HZ","6C","2","08"]
[null,null,null,null,null,null,"I1","BAT-K0000-216-1","1-2X16 SPLICE/SPLICE","I1","00","2","16"]
[null,null,null,null,null,null,"I2","BAT-K0022-216-1","1-2X16 SPLICE/LCAPC","I2","22","2","16"]
[null,null,null,null,null,null,"I3","BAT-K0044-216-1","1-2X16 SPLICE/SCAPC","I3","6C","2","16"]
[null,null,null,null,null,null,"I4","BAT-K2200-216-1","1-2X16 LCAPC/SPLICE","I4","00","2","16"]
[null,null,null,null,null,null,"I5","BAT-K2222-216-1","1-2X16 LCAPC/LCAPC","I5","22","2","16"]
[null,null,null,null,null,null,"I6","BAT-K2244-216-1","1-2X16 LCAPC/SCAPC","I6","6C","2","16"]
[null,null,null,null,null,null,"I7","BAT-K4400-216-1","1-2X16 SCAPC/SPLICE","I7","00","2","16"]
[null,null,null,null,null,null,"I8","BAT-K4422-216-1","1-2X16 SCAPC/LCAPC","I8","22","2","16"]
[null,null,null,null,null,null,"I9","BAT-K4444-216-1","1-2X16 SCAPC/SCAPC","I9","6C","2","16"]
[null,null,null,null,null,null,"J1","BAT-K0000-232-1","1-2X32 SPLICE/SPLICE","J1","00","2","32"]
[null,null,null,null,null,null,"J2","BAT-K0022-232-1","1-2X32 SPLICE/LCAPC","J2","22","2","32"]
[null,null,null,null,null,null,"J3","BAT-K0044-232-1","1-2X32 SPLICE/SCAPC","J3","6C","2","32"]
[null,null,null,null,null,null,"J4","BAT-K2200-232-1","1-2X32 LCAPC/SPLICE","J4","00","2","32"]
[null,null,null,null,null,null,"J5","BAT-K2222-232-1","1-2X32 LCAPC/LCAPC","J5","22","2","32"]
[null,null,null,null,null,null,"J6","BAT-K2244-232-1","1-2X32 LCAPC/SCAPC","J6","6C","2","32"]
[null,null,null,null,null,null,"J7","BAT-K4400-232-1","1-2X32 SCAPC/SPLICE","J7","00","2","32"]
[null,null,null,null,null,null,"J8","BAT-K4422-232-1","1-2X32 SCAPC/LCAPC","J8","22","2","32"]
[null,null,null,null,null,null,"J9","BAT-K4444-232-1","1-2X32 SCAPC/SCAPC","J9","6C","2","32"]
[null,null,null,null,null,null,"K1","BAT-K4444-264-1","1-2X64 SCAPC/SCAPC","K1","6C","2","64"]
[null,null,null,null,null,null,"K2","BAT-K0044-264-1","1-2X64 SPLICE/SCAPC","K2","6C","2","64"]
[null,null,null,null,null,null,"K3","BAT-K0022-264-1","1-2X64 SPLICE/LCAPC","K3",22,"2","64"]
[null,null,null,null,null,null,"K4","BAT-K2222-264-1","1-2X64 LCAPC/LCAPC","K4",22,"2","64"]
[null,null,null,null,null,null,"K5","BAT-K0000-264-1","1-2X64 SPLICE/SPLICE","K5",22,"2","64"]

{"sheet":"Data","index":2,"n_rows":262,"n_cols":29,"rows_kept":262,"cut":false,"hidden":true,"merged":[[10,24,10,26],[10,27,10,29],[10,21,10,23],[10,0,10,5],[10,6,10,8],[10,9,10,11],[10,12,10,14],[10,15,10,17],[10,18,10,19]]}
[]
["BPEOSIZES"]
["blank"]
["S0"]
["S1"]
["S1.5"]
["S2"]
["S3"]
[]
[]
["Evolv Drops",null,null,null,null,null,"Splitter",null,null,"2 to 8 Ports Pushlok and Stubbed SST",null,null,"2 to 8 Ports Pushlok and Stubbed SST with Optitip",null,null,"2 Rows of 4 ports Evolv Pushlok and Stubbed SST",null,null,"2 Rows of 4 ports  Evolv Pushlok and Stubbed SST with Optitip",null,null,"MINIXTEND ",null,null,"2 rows MINIXTEND ",null,null,"Accessories"]
["Evolv™ ROC™ Drop with Pushlok™ Technology, Dielectric ",null,null,"Evolv™ DualDrop™ Cable Assembly with Pushlok™ Technology",null,null,"Evolv™ Splitter Terminals with Pushlok™ Technology",null,null,"Evolv™ Terminals with Pushlok™ Technology, Stubbed SST ",null,null,"Evolv™ Terminals with Pushlok™ Technology, Stubbed SST with OptiTip® ",null,null,"Evolv™ Terminals with Pushlok™ Technology, 2 Rows , Stubbed SST",null,null,"Evolv™ Terminals with Pushlok™ Technology, 2 Rows ,  Stubbed SST with OptiTip® ",null,null,"Evolv™ Terminals with Pushlok™ Technology, Stubbed MiniXtend",null,null,"Evolv™ Terminals with Pushlok™ Technology, 2 Rows, Stubbed MiniXtend",null,null,"Evolv™ Terminals Accessories"]
["Part Number (blank)","Description (blank)",null,"Part Number (blank)","Description (blank)",null,"Part Number (blank)","Description (blank)",null,"Part Number (blank)","Description (blank)",null,"Part Number (blank)","Description (blank)",null,"Part Number (blank)","Description (blank)",null,"Part Number (blank)","Description (blank)",null,"Part Number (blank)","Description (blank)",null,"Part Number (blank)","Description (blank)",null,"Part Number (blank)","Description (blank)"]
["00D101JB49R030M","Evolv™ ROC™ Drop Assembly, Pushlok™ Pigtail, dielectric, 30 m, bulk packaging",null,"00D101JFDT3030M","Evolv™ DualDrop™ Cable Assembly, Pushlok™ Pigtail, 30 m, bulk packaging",null,"DSH4F100D1NC000S0P","Evolv™ Splitter Terminal with Pushlok™ Technology, 4 port, unstubbed, 1x4 splitter",null,"DMA2F1FDD1NC010M0P","Evolv™ Terminal with Pushlok™ Technology, 2 port, stubbed, SST Dielectric, 10 m",null,"DFA2F1FDD1M1003M0P","Evolv™ Terminal with Pushlok™ Technology, 2 port, preconnectorized OptiTip® stub, SST Dielectric, 3 m",null,"DMB4F1FDD1NC015M0P","Evolv™ Terminal with Pushlok Technology, 8 port, 2 rows of 4 ports, stubbed, SST Dielectric, 15 m",null,"DFB4F1FDD1M1015M0P","Evolv™ Terminal with Pushlok Technology, 8 port, 2 rows of 4 ports, preconnectorized OptiTip stub, SST Dielectric, 15 m",null,"DMA2F1MLD1NC015M0P","Evolv™ Terminal with Pushlok Technology, 2 port, stubbed, MiniXtend, 15 m",null,"DMB4F1MLD1NC015M0P","Evolv™ Terminal with Pushlok Technology, 8 port, 2 rows of 4 ports, stubbed, MiniXtend, 15 m",null,"CLEANER-PUSHLOK","Evolv™ Port Cleaner with Pushlok™ Technology, over 525 cleanings, compatible with both Pushlok™ and OptiTap® connectors and ports"]
["00D101EB49R030M-P","Evolv™ ROC™ Drop Assembly, Pushlok™ Pigtail, dielectric, 30 m, individual packaging",null,"00D101JFDT3030M-P","Evolv™ DualDrop™ Cable Assembly, Pushlok™ Pigtail, 30 m, individual packaging",null,"DSF8F100D1NC000S0P","Evolv™ Splitter Terminal with Pushlok™ Technology, 8 port, unstubbed, 1x8 splitter",null,"DMA2F1FDD1NC050M0P","Evolv™ Terminal with Pushlok™ Technology, 2 port, stubbed, SST Dielectric, 50 m",null,"DFA2F1FDD1M1015M0P","Evolv™ Terminal with Pushlok™ Technology, 2 port, preconnectorized OptiTip® stub, SST Dielectric, 15 m",null,"DMB4F1FDD1NC030M0P","Evolv™ Terminal with Pushlok Technology, 8 port, 2 rows of 4 ports, stubbed, SST Dielectric, 30 m",null,"DFB4F1FDD1M1030M0P","Evolv™ Terminal with Pushlok Technology, 8 port, 2 rows of 4 ports, preconnectorized OptiTip stub, SST Dielectric, 30 m",null,"DMA2F1MLD1NC030M0P","Evolv™ Terminal with Pushlok Technology, 2 port, stubbed, MiniXtend, 30 m",null,"DMB4F1MLD1NC030M0P","Evolv™ Terminal with Pushlok Technology, 8 port, 2 rows of 4 ports, stubbed, MiniXtend, 30 m",null,"KT-PL-SHROUD-SC","Evolv™ SC Converter with Pushlok™ Technology, used to convert Pushlok™ connectors to SC form factors, MOQ of 10"]
["00D101EB49R100M","Evolv™ ROC™ Drop Assembly, Pushlok™ Pigtail, dielectric, 100 m, bulk packaging",null,"00D101JFDT3050M","Evolv™ DualDrop™ Cable Assembly, Pushlok™ Pigtail, 50 m, bulk packaging",null,"DSF9F100D1NC000S0P","Evolv™ Splitter Terminal with Pushlok™ Technology, 8 port (2 rows of 4 ports), unstubbed, 1x8 splitter",null,"DMA2F1FDD1NC100M0P","Evolv™ Terminal with Pushlok™ Technology, 2 port, stubbed, SST Dielectric, 100 m",null,"DFA2F1FDD1M1030M0P","Evolv™ Terminal with Pushlok™ Technology, 2 port, preconnectorized OptiTip® stub, SST Dielectric, 30 m",null,"DMB4F1FDD1NC150M0P","Evolv™ Terminal with Pushlok Technology, 8 port, 2 rows of 4 ports, stubbed, SST Dielectric, 150 m",null,"DFB4F1FDD1M1150M0P","Evolv™ Terminal with Pushlok Technology, 8 port, 2 rows of 4 ports, preconnectorized OptiTip stub, SST Dielectric, 150 m",null,"DMA2F1MLD1NC150M0P","Evolv™ Terminal with Pushlok Technology, 2 port, stubbed, MiniXtend, 150 m",null,"DMB4F1MLD1NC150M0P","Evolv™ Terminal with Pushlok Technology, 8 port, 2 rows of 4 ports, stubbed, MiniXtend, 150 m",null,"KT-PL-OPT-CONV","Evolv™ OptiTap® Converter with Pushlok™ Technology, used to convert Pushlok™ connectors to OptiTap form factors (to plug into MultiPorts), MOQ of 10"]
["00D101EB49R100M-P","Evolv™ ROC™ Drop Assembly, Pushlok™ Pigtail, dielectric, 100 m, individual packaging",null,"00D101JFDT3050M-P","Evolv™ DualDrop™ Cable Assembly, Pushlok™ Pigtail, 50 m, individual packaging",null,"DSP6F100D1NC000S0P","Evolv™ Splitter Terminal with Pushlok™ Technology, 16 port (2 rows of 8 ports), unstubbed, 1x16 splitter",null,"DMA2F1FDD1NC150M0P","Evolv™ Terminal with Pushlok™ Technology, 2 port, stubbed, SST Dielectric, 150 m",null,"DFA2F1FDD1M1150M0P","Evolv™ Terminal with Pushlok™ Technology, 2 port, preconnectorized OptiTip® stub, SST Dielectric, 150 m",null,"DMB6F1FDD1NC015M0P","Evolv™ Terminal with Pushlok Technology, 12 port, 2 rows of 6 ports, stubbed, SST Dielectric, 15 m",null,"DFB6F1FDD1M1015M0P","Evolv™ Terminal with Pushlok Technology, 12 port, 2 rows of 6 ports, preconnectorized OptiTip stub, SST Dielectric, 15 m",null,"DMA4F1MLD1NC015M0P","Evolv™ Terminal with Pushlok Technology, 4 port, stubbed, MiniXtend, 15 m",null,"DMB6F1MLD1NC015M0P","Evolv™ Terminal with Pushlok Technology, 12 port, 2 rows of 6 ports, stubbed, MiniXtend, 15 m",null,"EHC-BKT-STRAND","Evolv™ Strand-Mount Bracket, compatible with all Evolv terminals (2, 4, 6 ,8, 12 and 16 port)"]
["00D101EB49R200M","Evolv™ ROC™ Drop Assembly, Pushlok™ Pigtail, dielectric, 200 m, bulk packaging",null,"00D101JFDT3080M","Evolv™ DualDrop™ Cable Assembly, Pushlok™ Pigtail, 80 m, bulk packaging",null,null,null,null,"DMA2F1FDD1NC200M0P","Evolv™ Terminal with Pushlok™ Technology, 2 port, stubbed, SST Dielectric, 200 m",null,"DFA4F1FDD1M1003M0P","Evolv™ Terminal with Pushlok™ Technology, 4 port, preconnectorized OptiTip® stub, SST Dielectric, 3 m",null,"DMB6F1FDD1NC030M0P","Evolv™ Terminal with Pushlok Technology, 12 port, 2 rows of 6 ports, stubbed, SST Dielectric, 30 m",null,"DFB6F1FDD1M1030M0P","Evolv™ Terminal with Pushlok Technology, 12 port, 2 rows of 6 ports, preconnectorized OptiTip stub, SST Dielectric, 30 m",null,"DMA4F1MLD1NC030M0P","Evolv™ Terminal with Pushlok Technology, 4 port, stubbed, MiniXtend, 30 m",null,"DMB6F1MLD1NC030M0P","Evolv™ Terminal with Pushlok Technology, 12 port, 2 rows of 6 ports, stubbed, MiniXtend, 30 m",null,"EHC-BKT-WALL","Evolv™ Wall- and Pole-Mount Bracket, compatible with 8-, 12- and 16-distribution port Evolv terminals (2 rows of ports)"]
["00D101EB49R200M-P","Evolv™ ROC™ Drop Assembly, Pushlok™ Pigtail, dielectric, 200 m, individual packaging",null,"00D101JFDT3080M-P","Evolv™ DualDrop™ Cable Assembly, Pushlok™ Pigtail, 80 m, individual packaging",null,null,null,null,"DMA2F1FDD1NC250M0P","Evolv™ Terminal with Pushlok™ Technology, 2 port, stubbed, SST Dielectric, 250 m",null,"DFA4F1FDD1M1015M0P","Evolv™ Terminal with Pushlok™ Technology, 4 port, preconnectorized OptiTip® stub, SST Dielectric, 15 m",null,"DMB6F1FDD1NC150M0P","Evolv™ Terminal with Pushlok Technology, 12 port, 2 rows of 6 ports, stubbed, SST Dielectric,  150 m",null,"DFB6F1FDD1M1150M0P","Evolv™ Terminal with Pushlok Technology, 12 port, 2 rows of 6 ports, preconnectorized OptiTip stub, SST Dielectric, 150 m",null,"DMA4F1MLD1NC150M0P","Evolv™ Terminal with Pushlok Technology, 4 port, stubbed, MiniXtend, 150 m",null,"DMB6F1MLD1NC150M0P","Evolv™ Terminal with Pushlok Technology, 12 port, 2 rows of 6 ports, stubbed, MiniXtend, 150 m",null,"EHC-BKT-HH","Evolv™ Handhole-Mount Bracket, compatible with all Evolv terminals (2, 4, 6 ,8, 12 and 16 port)"]
["00D101EB49R300M","Evolv™ ROC™ Drop Assembly, Pushlok™ Pigtail, dielectric, 300 m, bulk packaging",null,"00D101JFDT3100M","Evolv™ DualDrop™ Cable Assembly, Pushlok™ Pigtail, 100 m, bulk packaging",null,null,null,null,"DMA2F1FDD1NC300M0P","Evolv™ Terminal with Pushlok™ Technology, 2 port, stubbed, SST Dielectric, 300 m",null,"DFA4F1FDD1M1030M0P","Evolv™ Terminal with Pushlok™ Technology, 4 port, preconnectorized OptiTip® stub, SST Dielectric, 30 m",null,"DMB8F1FDD1NC015M0P","Evolv™ Terminal with Pushlok Technology, 16 port, 2 rows of 8 ports, stubbed, SST Dielectric, 15  m",null,null,null,null,"DMA6F1MLD1NC015M0P","Evolv™ Terminal with Pushlok Technology, 6 port, stubbed, MiniXtend, 15 m",null,"DMB8F1MLD1NC015M0P ","Evolv™ Terminal with Pushlok Technology, 16 port, 2 rows of 8 ports, stubbed, MiniXtend, 15 m",null,"EHC-CVR-A8-GRAY","Evolv™ 6- and 8-port Terminal Cover, compatible with 6- and 8-port Evolv terminals (single row of ports)"]
["00D101EB49R300M-P","Evolv™ ROC™ Drop Assembly, Pushlok™ Pigtail, dielectric, 300 m, individual packaging",null,"00D101JFDT3100M-P","Evolv™ DualDrop™ Cable Assembly, Pushlok™ Pigtail, 100 m, individual packaging",null,null,null,null,"DMA2F1FDD1NC350M0P","Evolv™ Terminal with Pushlok™ Technology, 2 port, stubbed, SST Dielectric, 350 m",null,"DFA4F1FDD1M1150M0P","Evolv™ Terminal with Pushlok™ Technology, 4 port, preconnectorized OptiTip® stub, SST Dielectric, 150 m",null,"DMB8F1FDD1NC030M0P","Evolv™ Terminal with Pushlok Technology, 16 port, 2 rows of 8 ports, stubbed, SST Dielectric, 30 m",null,null,null,null,"DMA6F1MLD1NC030M0P","Evolv™ Terminal with Pushlok Technology, 6 port, stubbed, MiniXtend, 30 m",null,"DMB8F1MLD1NC030M0P ","Evolv™ Terminal with Pushlok Technology, 16 port, 2 rows of 8 ports, stubbed, MiniXtend, 30 m",null,"EHC-CVR-A4-GRAY","Evolv™ 2- and 4-port Terminal Cover, compatible with 2- and 4-port Evolv terminals (single row of ports)"]
["D14401EB4R3030M","Evolv™ ROC™ Drop Assembly, Pushlok™ Hybrid Jumper, dielectric, 30 m, bulk packaging",null,"00D101JFDT3150M","Evolv™ DualDrop™ Cable Assembly, Pushlok™ Pigtail, 150 m, bulk packaging",null,null,null,null,"DMA4F1FDD1NC010M0P","Evolv™ Terminal with Pushlok™ Technology, 4 port, stubbed, SST Dielectric, 10 m",null,"DFA6F1FDD1M1003M0P","Evolv™ Terminal with Pushlok™ Technology, 6 port, preconnectorized OptiTip® stub, SST Dielectric, 3 m",null,"DMB8F1FDD1NC150M0P","Evolv™ Terminal with Pushlok Technology, 16 port, 2 rows of 8 ports, stubbed, SST Dielectric, 150 m",null,null,null,null,"DMA6F1MLD1NC150M0P","Evolv™ Terminal with Pushlok Technology, 6 port, stubbed, MiniXtend, 150 m",null,"DMB8F1MLD1NC150M0P ","Evolv™ Terminal with Pushlok Technology, 16 port, 2 rows of 8 ports, stubbed, MiniXtend, 150 m"]
["D14401EB4R3030M-P","Evolv™ ROC™ Drop Assembly, Pushlok™ Hybrid Jumper, dielectric, 30 m, individual packaging",null,"00D101JFDT3150M-P","Evolv™ DualDrop™ Cable Assembly, Pushlok™ Pigtail, 150 m, individual packaging",null,null,null,null,"DMA4F1FDD1NC050M0P","Evolv™ Terminal with Pushlok™ Technology, 4 port, stubbed, SST Dielectric, 50 m",null,"DFA6F1FDD1M1015M0P","Evolv™ Terminal with Pushlok™ Technology, 6 port, preconnectorized OptiTip® stub, SST Dielectric, 15 m",null,null,null,null,null,null,null,"DMA8F1MLD1NC015M0P","Evolv™ Terminal with Pushlok Technology, 8 port, stubbed, MiniXtend, 15 m"]
["D14401EB4R3100M","Evolv™ ROC™ Drop Assembly, Pushlok™ Hybrid Jumper, dielectric, 100 m, bulk packaging",null,null,null,null,null,null,null,"DMA4F1FDD1NC100M0P","Evolv™ Terminal with Pushlok™ Technology, 4 port, stubbed, SST Dielectric, 100 m",null,"DFA6F1FDD1M1030M0P","Evolv™ Terminal with Pushlok™ Technology, 6 port, preconnectorized OptiTip® stub, SST Dielectric, 30 m",null,null,null,null,null,null,null,"DMA8F1MLD1NC030M0P","Evolv™ Terminal with Pushlok Technology, 8 port, stubbed, MiniXtend, 30 m"]
["D14401EB4R3100M-P","Evolv™ ROC™ Drop Assembly, Pushlok™ Hybrid Jumper, dielectric, 100 m, individual packaging",null,null,null,null,null,null,null,"DMA4F1FDD1NC150M0P","Evolv™ Terminal with Pushlok™ Technology, 4 port, stubbed, SST Dielectric, 150 m",null,"DFA6F1FDD1M1150M0P","Evolv™ Terminal with Pushlok™ Technology, 6 port, preconnectorized OptiTip® stub, SST Dielectric, 150 m",null,null,null,null,null,null,null,"DMA8F1MLD1NC150M0P","Evolv™ Terminal with Pushlok Technology, 8 port, stubbed, MiniXtend, 150 m"]
["D14401EB4R3200M","Evolv™ ROC™ Drop Assembly, Pushlok™ Hybrid Jumper, dielectric, 200 m, bulk packaging",null,null,null,null,null,null,null,"DMA4F1FDD1NC200M0P","Evolv™ Terminal with Pushlok™ Technology, 4 port, stubbed, SST Dielectric, 200 m",null,"DFA8F1FDD1M1003M0P","Evolv™ Terminal with Pushlok™ Technology, 8 port, preconnectorized OptiTip® stub, SST Dielectric, 3 m"]
["D14401EB4R3200M-P","Evolv™ ROC™ Drop Assembly, Pushlok™ Hybrid Jumper, dielectric, 200 m, individual packaging",null,null,null,null,null,null,null,"DMA4F1FDD1NC250M0P","Evolv™ Terminal with Pushlok™ Technology, 4 port, stubbed, SST Dielectric, 250 m",null,"DFA8F1FDD1M1015M0P","Evolv™ Terminal with Pushlok™ Technology, 8 port, preconnectorized OptiTip® stub, SST Dielectric, 15 m"]
["D14401EB49R300M","Evolv™ ROC™ Drop Assembly, Pushlok™ Hybrid Jumper, dielectric, 300 m, bulk packaging",null,null,null,null,null,null,null,"DMA4F1FDD1NC300M0P","Evolv™ Terminal with Pushlok™ Technology, 4 port, stubbed, SST Dielectric, 300 m",null,"DFA8F1FDD1M1030M0P","Evolv™ Terminal with Pushlok™ Technology, 8 port, preconnectorized OptiTip® stub, SST Dielectric, 30 m"]
["D14401EB49R300M-P","Evolv™ ROC™ Drop Assembly, Pushlok™ Hybrid Jumper, dielectric, 300 m, individual packaging",null,null,null,null,null,null,null,"DMA4F1FDD1NC350M0P","Evolv™ Terminal with Pushlok™ Technology, 4 port, stubbed, SST Dielectric, 350 m",null,"DFA8F1FDD1M1150M0P","Evolv™ Terminal with Pushlok™ Technology, 8 port, preconnectorized OptiTip® stub, SST Dielectric, 150 m"]
["D1D101EB49R030M","Evolv™ ROC™ Drop Assembly, Pushlok™ Jumper, dielectric, 30 m, bulk packaging",null,null,null,null,null,null,null,"DMA6F1FDD1NC010M0P","Evolv™ Terminal with Pushlok™ Technology, 6 port, stubbed, SST Dielectric, 10 m"]
["D1D101EB49R030M-P","Evolv™ ROC™ Drop Assembly, Pushlok™ Jumper, dielectric, 30 m, individual packaging",null,null,null,null,null,null,null,"DMA6F1FDD1NC050M0P","Evolv™ Terminal with Pushlok™ Technology, 6 port, stubbed, SST Dielectric, 50 m"]
["D1D101EB49R100M","Evolv™ ROC™ Drop Assembly, Pushlok™ Jumper, dielectric, 100 m, bulk packaging",null,null,null,null,null,null,null,"DMA6F1FDD1NC100M0P","Evolv™ Terminal with Pushlok™ Technology, 6 port, stubbed, SST Dielectric, 100 m"]
["D1D101EB49R100M-P","Evolv™ ROC™ Drop Assembly, Pushlok™ Jumper, dielectric, 100 m, individual packaging",null,null,null,null,null,null,null,"DMA6F1FDD1NC150M0P","Evolv™ Terminal with Pushlok™ Technology, 6 port, stubbed, SST Dielectric, 150 m"]
["D1D101EB49R200M","Evolv™ ROC™ Drop Assembly, Pushlok™ Jumper, dielectric, 200 m, bulk packaging",null,null,null,null,null,null,null,"DMA6F1FDD1NC200M0P","Evolv™ Terminal with Pushlok™ Technology, 6 port, stubbed, SST Dielectric, 200 m"]
["D1D101EB49R200M-P","Evolv™ ROC™ Drop Assembly, Pushlok™ Jumper, dielectric, 200 m, individual packaging",null,null,null,null,null,null,null,"DMA6F1FDD1NC250M0P","Evolv™ Terminal with Pushlok™ Technology, 6 port, stubbed, SST Dielectric, 250 m"]
["D1D101EB49R300M","Evolv™ ROC™ Drop Assembly, Pushlok™ Jumper, dielectric, 300 m, bulk packaging",null,null,null,null,null,null,null,"DMA6F1FDD1NC300M0P","Evolv™ Terminal with Pushlok™ Technology, 6 port, stubbed, SST Dielectric, 300 m"]
["D1D101EB49R300M-P","Evolv™ ROC™ Drop Assembly, Pushlok™ Jumper, dielectric, 300 m, individual packaging",null,null,null,null,null,null,null,"DMA6F1FDD1NC350M0P","Evolv™ Terminal with Pushlok™ Technology, 6 port, stubbed, SST Dielectric, 350 m"]
[null,null,null,null,null,null,null,null,null,"DMA8F1FDD1NC010M0P","Evolv™ Terminal with Pushlok™ Technology, 8 port, stubbed, SST Dielectric, 10 m"]
[null,null,null,null,null,null,null,null,null,"DMA8F1FDD1NC050M0P","Evolv™ Terminal with Pushlok™ Technology, 8 port, stubbed, SST Dielectric, 50 m"]
[null,null,null,null,null,null,null,null,null,"DMA8F1FDD1NC100M0P","Evolv™ Terminal with Pushlok™ Technology, 8 port, stubbed, SST Dielectric, 100 m"]
[null,null,null,null,null,null,null,null,null,"DMA8F1FDD1NC150M0P","Evolv™ Terminal with Pushlok™ Technology, 8 port, stubbed, SST Dielectric, 150 m"]
[null,null,null,null,null,null,null,null,null,"DMA8F1FDD1NC200M0P","Evolv™ Terminal with Pushlok™ Technology, 8 port, stubbed, SST Dielectric, 200 m"]
[null,null,null,null,null,null,null,null,null,"DMA8F1FDD1NC250M0P","Evolv™ Terminal with Pushlok™ Technology, 8 port, stubbed, SST Dielectric, 250 m"]
[null,null,null,null,null,null,null,null,null,"DMA8F1FDD1NC300M0P","Evolv™ Terminal with Pushlok™ Technology, 8 port, stubbed, SST Dielectric, 300 m"]
[null,null,null,null,null,null,null,null,null,"DMA8F1FDD1NC350M0P","Evolv™ Terminal with Pushlok™ Technology, 8 port, stubbed, SST Dielectric, 350 m"]
[]
[]
[]
[]
[]
["BoM BAT"]
[]
[null,null,null,null,null,null,null,null,null,null,"Size S","Size M"]
["Cable Entry",null,null,null,"ACTIVE IN PCN AND IN CONFIGURATOR BOM",null,null,null,null,null,null,null,"BAT-CC8-10","BAT KIT -STRAIN RELIEF 8MM BP10","A","A- Cables with aramid yarn up to 8mm and Pixian"]
["A","BAT-CC8-01","BAT KIT -STRAIN RELIEF 8MM SP","A","BAT-CC8-10","BAT KIT -STRAIN RELIEF 8MM BP10",null,"Cables with aramid yarn up to 8mm and Pixian",null,null,null,null,"BAT-CLT-01","BAT KIT - FANOUT FOR LT 3MM 10pcs SP","B","B- Fan-out"]
["B","BAT-CLT-01","BAT KIT - FANOUT FOR LT 3MM 10pcs SP","B","BAT-CLT-01","BAT KIT - FANOUT FOR LT 3MM 10pcs SP",null,"Fan-out",null,null,null,null,"BAT-CDM-01","BAT(M) Kit-Strain relief 8 and 12mm","C","C- Cables + ducts up to 12 mm"]
["C","BAT-CM1-01","BAT KIT - METAL INNER STRAIN RELIEF SP","C","xxx","xxx",null,"xx",null,null,null,null,"BAT-CAM-01","BAT(M) KIT- Str. Rel. Cable w/ Cent. Me","D","D- Cable with central member or with fucation adapter"]
["D","BAT-CDM-01","BAT (M) KIT -DUCT STRAIN RELIEF 8MM SP","D","BAT-CDM-01","BAT(M) Kit-Strain relief 8 and 12mm",null,"Cables + ducts up to 12 mm",null,null,null,null,"BAT-CFM-01","BAT Sealing foam kit - M size (1x12 or 4x8mm)","E","E- Sealing Foam option"]
["E","BAT-CDX-01","BAT (L/X) KIT - DUCT STRN REL 8MM R SP","E","BAT-CDX-01","BAT(L/X) Kit-Strain relief 8 and12mm"]
["F","BAT-CDY-01","BAT (L/X) KIT - DUCT STRN REL 8MM L SP","F","BAT-CDL-01","BAT(L) KIT STRAIN RELIEF 8 AND 12 MM"]
["G","BAT-CTM-01","BAT (M) KIT - DUCT STRAIN REL 12MM SP","G","BAT-CFT-01","BAT Sealing foam kit – L/X size (2x2 12mm)"]
["H","BAT-CTP-01","BAT (L/XL) KIT - PG GLAND M20 SP","H","BAT-CTP-01","BAT (L,X) Kit - PG Gland 13-18mm"]
["I","BAT-CTX-01","BAT (L/X) KIT -DUCT STRN REL 12MM R SP","I","OBS"]
["J","BAT-CTY-01","BAT (L/X) KIT -DUCT STRN REL 12MM L SP","J","BAT-CFS-01","BAT Sealing foam kit - S size (1x12 or 4x8mm)"]
["K","BAT-CXL-01","BAT(L) KIT – PIXIAN STRAIN RELIEF","K","BAT-CFM-01","BAT Sealing foam kit - M size (1x12 or 4x8mm)"]
["L","BAT-CXX-01","BAT(X) KIT – PIXIAN STRAIN RELIEF","L","BAT-CFX-01","BAT Sealing foam kit – X size (2x 12mm)"]
["M","BAT-CXM-01","BAT(X) KIT – PIXIAN STRAIN RELIEF","M","BAT-CFY-01","BAT Sealing foam kit – L/X size (2x2 8mm)"]
["N","BAT-CDL-01","BAT(L) KIT STRAIN RELIEF 8 AND 12 MM","N","BAT-CFZ-01","BAT Sealing foam kit – L/X size (4x4 8mm)"]
["O","BAT-CAM-01","Cable with central member or with furcation adapter","O"]
["P","BAT-CAL-01","Cable with central member or with furcation adapter","P","ACTIVE IN PCN NOT IN CONFIGURATOR BOM"]
["Q","BAT-CAX-01","Cable with central member or with furcation adapter","Q","BAT-CAM-01","BAT(M) KIT- Str. Rel. Cable w/ Cent. Me",null,"Cable with central member or with fucation adapter"]
[]
[null,null,null,null,"BAT-CAX-01","BAT(X) KIT STRAIN RELIEF 8 AND 12 MM"]
[null,null,null,null,"BAT-CFS-01","BAT Sealing foam kit - S size (1x12 or 2x8mm)"]
[]
[null,null,null,null,"BAT-CXL-01","BAT(L) KIT – PIXIAN STRAIN RELIEF"]
[1,"BAT-CFM-01","BAT (M) KIT -SEALING FOAM I/O 12MM SP",1,"BAT-CXX-01","BAT(X) KIT – PIXIAN STRAIN RELIEF"]
[2,"BAT-CFX-01","BAT (L/X)KIT -SEALING FOAM OUT 12MM SP",2,"BAT-CXM-01","BAT(X) KIT – PIXIAN STRAIN RELIEF"]
[3,"BAT-CFY-01","BAT (L) KIT -SEALING FOAM IN 12MM SP",3]
[4,"BAT-CFZ-01","BAT (X) KIT -SEALING FOAM IN 12MM SP",4]
[5,"BAT-CFT-01","BAT Sealing foam kit – L/X size (2x2 12mm)",5]
[null,null,null,null,"OBSOLETED IN PCN"]
[null,null,null,null,"BAT-CAL-01"]
[null,null,null,null,"BAT-CCE-01"]
[null,null,null,null,"BAT-CDY-01"]
[null,null,null,null,"BAT-CM1-01"]
[null,null,null,null,"BAT-CTM-01"]
[null,null,null,null,"BAT-CTS-01"]
[null,null,null,null,"BAT-CTX-01"]
[null,null,null,null,"BAT-CTY-01"]
[null,null,null,null,"BAT-CXL-01"]
[]
[]
[]
[]
[]
["BoM UNISUB HD"]
[]
["With Heathshrink Splice Trays (up to 96 splices per drawer)"]
["PGTL =","with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["Catalog Number","Short","Length of Short","Long"]
["UHD-1L-486C-PGTL","Unisub HD 1U Left 48 SC/APC Telcordia",37,"Unisub HD 1U Left 48 ports, 48 SC/APC simplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-1L-726C-PGTL","Unisub HD 1U Left 72 SC/APC Telcordia",37,"Unisub HD 1U Left 72 ports, 72 SC/APC simplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-1L-7222-PGTL","Unisub HD 1U Left 72 LC/APC Telcordia",37,"Unisub HD 1U Left 72 ports, 36 LC/APC duplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-1L-96B3-PGTL","Unisub HD 1U Left 96 LCAshut Telcordia",38,"Unisub HD 1U Left 96 ports, 48 LC/APC shuttered duplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-2L-486C-PGTL","Unisub HD 2U Left 96 SC/APC Telcordia",37,"Unisub HD 2U Left 96 ports, 96 SC/APC simplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-2L-726C-PGTL","Unisub HD 2U Left 144 SC/APC Telcordia",38,"Unisub HD 2U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-2L-7222-PGTL","Unisub HD 2U Left 144 LC/APC Telcordia",38,"Unisub HD 2U Left 144 ports, 72 LC/APC duplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-2L-96B3-PGTL","Unisub HD 2U Left 192 LCAshut Telcordia",39,"Unisub HD 2U Left 192 ports, 96 LC/APC shuttered duplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-3L-486C-PGTL","Unisub HD 3U Left 144 SC/APC Telcordia",38,"Unisub HD 3U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-3L-726C-PGTL","Unisub HD 3U Left 216 SC/APC Telcordia",38,"Unisub HD 3U Left 216 ports, 216 SC/APC simplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-3L-7222-PGTL","Unisub HD 3U Left 216 LC/APC Telcordia",38,"Unisub HD 3U Left 216 ports, 108 LC/APC duplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-3L-96B3-PGTL","Unisub HD 3U Left 288 LCAshut Telcordia",39,"Unisub HD 3U Left 288 ports, 144 LC/APC shuttered duplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-4L-486C-PGTL","Unisub HD 4U Left 192 SC/APC Telcordia",38,"Unisub HD 4U Left 192 ports, 192 SC/APC simplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-4L-726C-PGTL","Unisub HD 4U Left 288 SC/APC Telcordia",38,"Unisub HD 4U Left 288 ports, 288 SC/APC simplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-4L-7222-PGTL","Unisub HD 4U Left 288 LC/APC Telcordia",38,"Unisub HD 4U Left 288 ports, 144 LC/APC duplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-4L-96B3-PGTL","Unisub HD 4U Left 384 LCAshut Telcordia",39,"Unisub HD 4U Left 384 ports, 192 LC/APC shuttered duplex adapters, with Pigtails, Grade C, Telcordia Colour Coding, with Heatshrink splice trays"]
[]
["PGGB =","with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["Catalog Number","Short","Length of Short","Long"]
["UHD-1L-486C-PGGB","Unisub HD 1U Left 48 SC/APC GrB Telcord",39,"Unisub HD 1U Left 48 ports, 48 SC/APC simplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-1L-726C-PGGB","Unisub HD 1U Left 72 SC/APC GrB Telcord",39,"Unisub HD 1U Left 72 ports, 72 SC/APC simplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-1L-7222-PGGB","Unisub HD 1U Left 72 LC/APC GrB Telcord",39,"Unisub HD 1U Left 72 ports, 36 LC/APC duplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-1L-96B3-PGGB","Unisub HD 1U Left 96 LCAshut GrB Telcord",40,"Unisub HD 1U Left 96 ports, 48 LC/APC shuttered duplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-2L-486C-PGGB","Unisub HD 2U Left 96 SC/APC GrB Telcord",39,"Unisub HD 2U Left 96 ports, 96 SC/APC simplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-2L-726C-PGGB","Unisub HD 2U Left 144 SC/APC GrB Telcord",40,"Unisub HD 2U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-2L-7222-PGGB","Unisub HD 2U Left 144 LC/APC GrB Telcord",40,"Unisub HD 2U Left 144 ports, 72 LC/APC duplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-2L-96B3-PGGB","Unisub HD 2U Left 192 LCAshut GrB Telcor",40,"Unisub HD 2U Left 192 ports, 96 LC/APC shuttered duplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-3L-486C-PGGB","Unisub HD 3U Left 144 SC/APC GrB Telcord",40,"Unisub HD 3U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-3L-726C-PGGB","Unisub HD 3U Left 216 SC/APC GrB Telcord",40,"Unisub HD 3U Left 216 ports, 216 SC/APC simplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-3L-7222-PGGB","Unisub HD 3U Left 216 LC/APC GrB Telcord",40,"Unisub HD 3U Left 216 ports, 108 LC/APC duplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-3L-96B3-PGGB","Unisub HD 3U Left 288 LCAshut GrB Telcor",40,"Unisub HD 3U Left 288 ports, 144 LC/APC shuttered duplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-4L-486C-PGGB","Unisub HD 4U Left 192 SC/APC GrB Telcord",40,"Unisub HD 4U Left 192 ports, 192 SC/APC simplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-4L-726C-PGGB","Unisub HD 4U Left 288 SC/APC GrB Telcord",40,"Unisub HD 4U Left 288 ports, 288 SC/APC simplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-4L-7222-PGGB","Unisub HD 4U Left 288 LC/APC GrB Telcord",40,"Unisub HD 4U Left 288 ports, 144 LC/APC duplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
["UHD-4L-96B3-PGGB","Unisub HD 4U Left 384 LCAshut GrB Telcor",40,"Unisub HD 4U Left 384 ports, 192 LC/APC shuttered duplex adapters, with Pigtails, Grade B, Telcordia Colour Coding, with Heatshrink splice trays"]
[]
["PGFR =","with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["Catalog Number","Short","Length of Short"]
["UHD-1L-486C-PGFR","Unisub HD 1U Left 48 SC/APC Orange",34,"Unisub HD 1U Left 48 ports, 48 SC/APC simplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-1L-726C-PGFR","Unisub HD 1U Left 72 SC/APC Orange",34,"Unisub HD 1U Left 72 ports, 72 SC/APC simplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-1L-7222-PGFR","Unisub HD 1U Left 72 LC/APC Orange",34,"Unisub HD 1U Left 72 ports, 36 LC/APC duplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-1L-96B3-PGFR","Unisub HD 1U Left 96 LCAshut Orange",35,"Unisub HD 1U Left 96 ports, 48 LC/APC shuttered duplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-2L-486C-PGFR","Unisub HD 2U Left 96 SC/APC Orange",34,"Unisub HD 2U Left 96 ports, 96 SC/APC simplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-2L-726C-PGFR","Unisub HD 2U Left 144 SC/APC Orange",35,"Unisub HD 2U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-2L-7222-PGFR","Unisub HD 2U Left 144 LC/APC Orange",35,"Unisub HD 2U Left 144 ports, 72 LC/APC duplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-2L-96B3-PGFR","Unisub HD 2U Left 192 LCAshut Orange",36,"Unisub HD 2U Left 192 ports, 96 LC/APC shuttered duplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-3L-486C-PGFR","Unisub HD 3U Left 144 SC/APC Orange",35,"Unisub HD 3U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-3L-726C-PGFR","Unisub HD 3U Left 216 SC/APC Orange",35,"Unisub HD 3U Left 216 ports, 216 SC/APC simplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-3L-7222-PGFR","Unisub HD 3U Left 216 LC/APC Orange",35,"Unisub HD 3U Left 216 ports, 108 LC/APC duplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-3L-96B3-PGFR","Unisub HD 3U Left 288 LCAshut Orange",36,"Unisub HD 3U Left 288 ports, 144 LC/APC shuttered duplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-4L-486C-PGFR","Unisub HD 4U Left 192 SC/APC Orange",35,"Unisub HD 4U Left 192 ports, 192 SC/APC simplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-4L-726C-PGFR","Unisub HD 4U Left 288 SC/APC Orange",35,"Unisub HD 4U Left 288 ports, 288 SC/APC simplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-4L-7222-PGFR","Unisub HD 4U Left 288 LC/APC Orange",35,"Unisub HD 4U Left 288 ports, 144 LC/APC duplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-4L-96B3-PGFR","Unisub HD 4U Left 384 LCAshut Orange",36,"Unisub HD 4U Left 384 ports, 192 LC/APC shuttered duplex adapters, with Pigtails, Grade C, Orange France Colour Coding, with Heatshrink splice trays"]
[]
["PGBF =","with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["Catalog Number","Short","Length of Short"]
["UHD-1L-486C-PGBF","Unisub HD 1U Left 48 SC/APC GrB Orange",38,"Unisub HD 1U Left 48 ports, 48 SC/APC simplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-1L-726C-PGBF","Unisub HD 1U Left 72 SC/APC GrB Orange",38,"Unisub HD 1U Left 72 ports, 72 SC/APC simplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-1L-7222-PGBF","Unisub HD 1U Left 72 LC/APC GrB Orange",38,"Unisub HD 1U Left 72 ports, 36 LC/APC duplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-1L-96B3-PGBF","Unisub HD 1U Left 96 LCAshut GrB Orange",39,"Unisub HD 1U Left 96 ports, 48 LC/APC shuttered duplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-2L-486C-PGBF","Unisub HD 2U Left 96 SC/APC GrB Orange",38,"Unisub HD 2U Left 96 ports, 96 SC/APC simplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-2L-726C-PGBF","Unisub HD 2U Left 144 SC/APC GrB Orange",39,"Unisub HD 2U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-2L-7222-PGBF","Unisub HD 2U Left 144 LC/APC GrB Orange",39,"Unisub HD 2U Left 144 ports, 72 LC/APC duplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-2L-96B3-PGBF","Unisub HD 2U Left 192 LCAshut GrB Orange",40,"Unisub HD 2U Left 192 ports, 96 LC/APC shuttered duplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-3L-486C-PGBF","Unisub HD 3U Left 144 SC/APC GrB Orange",39,"Unisub HD 3U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-3L-726C-PGBF","Unisub HD 3U Left 216 SC/APC GrB Orange",39,"Unisub HD 3U Left 216 ports, 216 SC/APC simplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-3L-7222-PGBF","Unisub HD 3U Left 216 LC/APC GrB Orange",39,"Unisub HD 3U Left 216 ports, 108 LC/APC duplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-3L-96B3-PGBF","Unisub HD 3U Left 288 LCAshut GrB Orange",40,"Unisub HD 3U Left 288 ports, 144 LC/APC shuttered duplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-4L-486C-PGBF","Unisub HD 4U Left 192 SC/APC GrB Orange",39,"Unisub HD 4U Left 192 ports, 192 SC/APC simplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-4L-726C-PGBF","Unisub HD 4U Left 288 SC/APC GrB Orange",39,"Unisub HD 4U Left 288 ports, 288 SC/APC simplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-4L-7222-PGBF","Unisub HD 4U Left 288 LC/APC GrB Orange",39,"Unisub HD 4U Left 288 ports, 144 LC/APC duplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
["UHD-4L-96B3-PGBF","Unisub HD 4U Left 384 LCAshut GrB Orange",40,"Unisub HD 4U Left 384 ports, 192 LC/APC shuttered duplex adapters, with Pigtails, Grade B, Orange France Colour Coding, with Heatshrink splice trays"]
[]
["PCVH =","with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays "]
["Catalog Number","Short","Length of Short"]
["UHD-1L-486C-PCVH","Unisub HD 1U Left 48 SC/APC HS, VDE",35,"Unisub HD 1U Left 48 ports, 48 SC/APC simplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-1L-726C-PCVH","Unisub HD 1U Left 72 SC/APC HS, VDE",35,"Unisub HD 1U Left 72 ports, 72 SC/APC simplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-1L-7222-PCVH","Unisub HD 1U Left 72 LC/APC HS, VDE",35,"Unisub HD 1U Left 72 ports, 36 LC/APC duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-1L-96B3-PCVH","Unisub HD 1U Left 96 LCAshut HS, VDE",36,"Unisub HD 1U Left 96 ports, 48 LC/APC shuttered duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-2L-486C-PCVH","Unisub HD 2U Left 96 SC/APC HS, VDE",35,"Unisub HD 2U Left 96 ports, 96 SC/APC simplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-2L-726C-PCVH","Unisub HD 2U Left 144 SC/APC HS, VDE",36,"Unisub HD 2U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-2L-7222-PCVH","Unisub HD 2U Left 144 LC/APC HS, VDE",36,"Unisub HD 2U Left 144 ports, 72 LC/APC duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-2L-96B3-PCVH","Unisub HD 2U Left 192 LCAshut HS, VDE",37,"Unisub HD 2U Left 192 ports, 96 LC/APC shuttered duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-3L-486C-PCVH","Unisub HD 3U Left 144 SC/APC HS, VDE",36,"Unisub HD 3U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-3L-726C-PCVH","Unisub HD 3U Left 216 SC/APC HS, VDE",36,"Unisub HD 3U Left 216 ports, 216 SC/APC simplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-3L-7222-PCVH","Unisub HD 3U Left 216 LC/APC HS, VDE",36,"Unisub HD 3U Left 216 ports, 108 LC/APC duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-3L-96B3-PCVH","Unisub HD 3U Left 288 LCAshut HS, VDE",37,"Unisub HD 3U Left 288 ports, 144 LC/APC shuttered duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-4L-486C-PCVH","Unisub HD 4U Left 192 SC/APC HS, VDE",36,"Unisub HD 4U Left 192 ports, 192 SC/APC simplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-4L-726C-PCVH","Unisub HD 4U Left 288 SC/APC HS, VDE",36,"Unisub HD 4U Left 288 ports, 288 SC/APC simplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-4L-7222-PCVH","Unisub HD 4U Left 288 LC/APC HS, VDE",36,"Unisub HD 4U Left 288 ports, 144 LC/APC duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-4L-96B3-PCVH","Unisub HD 4U Left 384 LCAshut HS, VDE",37,"Unisub HD 4U Left 384 ports, 192 LC/APC shuttered duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Heathsrink splice trays"]
[]
["PBVH =","with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["Catalog Number","Short","Length of Short"]
["UHD-1L-486C-PCVH","Unisub HD 1U Left 48 SC/APC HS, GrB VDE",39,"Unisub HD 1U Left 48 ports, 48 SC/APC simplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-1L-726C-PCVH","Unisub HD 1U Left 72 SC/APC HS, GrB VDE",39,"Unisub HD 1U Left 72 ports, 72 SC/APC simplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-1L-7222-PCVH","Unisub HD 1U Left 72 LC/APC HS, GrB VDE",39,"Unisub HD 1U Left 72 ports, 36 LC/APC duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-1L-96B3-PCVH","Unisub HD 1U Left 96 LCAshut HS, GrB VDE",40,"Unisub HD 1U Left 96 ports, 48 LC/APC shuttered duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-2L-486C-PCVH","Unisub HD 2U Left 96 SC/APC HS, GrB VDE",39,"Unisub HD 2U Left 96 ports, 96 SC/APC simplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-2L-726C-PCVH","Unisub HD 2U Left 144 SC/APC HS, GrB VDE",40,"Unisub HD 2U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-2L-7222-PCVH","Unisub HD 2U Left 144 LC/APC HS, GrB VDE",40,"Unisub HD 2U Left 144 ports, 72 LC/APC duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-2L-96B3-PCVH","Unisub HD 2U Left 192 LCAshut HS GrB VDE",40,"Unisub HD 2U Left 192 ports, 96 LC/APC shuttered duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-3L-486C-PCVH","Unisub HD 3U Left 144 SC/APC HS, GrB VDE",40,"Unisub HD 3U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-3L-726C-PCVH","Unisub HD 3U Left 216 SC/APC HS, GrB VDE",40,"Unisub HD 3U Left 216 ports, 216 SC/APC simplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-3L-7222-PCVH","Unisub HD 3U Left 216 LC/APC HS, GrB VDE",40,"Unisub HD 3U Left 216 ports, 108 LC/APC duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-3L-96B3-PCVH","Unisub HD 3U Left 288 LCAshut HS GrB VDE",40,"Unisub HD 3U Left 288 ports, 144 LC/APC shuttered duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-4L-486C-PCVH","Unisub HD 4U Left 192 SC/APC HS, GrB VDE",40,"Unisub HD 4U Left 192 ports, 192 SC/APC simplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-4L-726C-PCVH","Unisub HD 4U Left 288 SC/APC HS, GrB VDE",40,"Unisub HD 4U Left 288 ports, 288 SC/APC simplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-4L-7222-PCVH","Unisub HD 4U Left 288 LC/APC HS, GrB VDE",40,"Unisub HD 4U Left 288 ports, 144 LC/APC duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
["UHD-4L-96B3-PCVH","Unisub HD 4U Left 384 LCAshut HS GrB VDE",40,"Unisub HD 4U Left 384 ports, 192 LC/APC shuttered duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Heathsrink splice trays"]
[]
["With Crimp Splice Trays (limited to 48 splices per drawer)"]
["PGVD =","with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays "]
["Catalog Number","Short","Length of Short"]
["UHD-1L-486C-PGVD","Unisub HD 1U Left 48 SC/APC crimp VDE",37,"Unisub HD 1U Left 48 ports, 48 SC/APC simplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-1L-4822-PGVD","Unisub HD 1U Left 48 LC/APC crimp VDE",37,"Unisub HD 1U Left 48 ports, 24 LC/APC duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-1L-48B3-PGVD","Unisub HD 1U Left 48 LCAshut crimp VDE",38,"Unisub HD 1U Left 48 ports, 24 LC/APC shuttered duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-2L-486C-PGVD","Unisub HD 2U Left 96 SC/APC crimp VDE",37,"Unisub HD 2U Left 96 ports, 96 SC/APC simplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-2L-4822-PGVD","Unisub HD 2U Left 96 SC/APC crimp VDE",37,"Unisub HD 2U Left 96 ports, 48 LC/APC duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-2L-48B3-PGVD","Unisub HD 2U Left 96 LC/APC crimp VDE",37,"Unisub HD 2U Left 96 ports, 48 LC/APC shuttered duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-3L-486C-PGVD","Unisub HD 3U Left 144 LCAshut crimp VDE",39,"Unisub HD 3U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-3L-4822-PGVD","Unisub HD 3U Left 144 SC/APC crimp VDE",38,"Unisub HD 3U Left 144 ports, 72 LC/APC duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-3L-48B3-PGVD","Unisub HD 3U Left 144 SC/APC crimp VDE",38,"Unisub HD 3U Left 144 ports, 72 LC/APC shuttered duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-4L-486C-PGVD","Unisub HD 4U Left 192 LC/APC crimp VDE",38,"Unisub HD 4U Left 192 ports, 192 SC/APC simplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-4L-4822-PGVD","Unisub HD 4U Left 192 LCAshut crimp VDE",39,"Unisub HD 4U Left 192 ports, 96 LC/APC duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-4L-48B3-PGVD","Unisub HD 4U Left 192 SC/APC crimp VDE",38,"Unisub HD 4U Left 192 ports, 96 LC/APC shuttered duplex adapters, with Pigtails, Grade C, VDE Germany Colour Coding, with Crimp splice trays"]
[]
["PBVD =","with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
["Catalog Number","Short","Length of Short"]
["UHD-1L-486C-PBVD","Unisub HD 1U Left 48 SCA crimp GrB VDE",38,"Unisub HD 1U Left 48 ports, 48 SC/APC simplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-1L-4822-PBVD","Unisub HD 1U Left 48 LCA crimp GrB VDE",38,"Unisub HD 1U Left 48 ports, 24 LC/APC duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-1L-48B3-PBVD","Unisub HD 1U Left 48 LCAsh crimp GrB VDE",40,"Unisub HD 1U Left 48 ports, 24 LC/APC shuttered duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-2L-486C-PBVD","Unisub HD 2U Left 96 SCA crimp GrB VDE",38,"Unisub HD 2U Left 96 ports, 96 SC/APC simplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-2L-4822-PBVD","Unisub HD 2U Left 96 LCA crimp GrB VDE",38,"Unisub HD 2U Left 96 ports, 48 LC/APC duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-2L-48B3-PBVD","Unisub HD 2U Left 96 LCAsh crimp GrB VDE",40,"Unisub HD 2U Left 96 ports, 48 LC/APC shuttered duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-3L-486C-PBVD","Unisub HD 3U Left 144 SCA crimp GrB VDE",39,"Unisub HD 3U Left 144 ports, 144 SC/APC simplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-3L-4822-PBVD","Unisub HD 3U Left 144 LCA crimp GrB VDE",39,"Unisub HD 3U Left 144 ports, 72 LC/APC duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-3L-48B3-PBVD","Unisub HD 3U Left 144 LCAsh crimp GB VDE",40,"Unisub HD 3U Left 144 ports, 72 LC/APC shuttered duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-4L-486C-PBVD","Unisub HD 4U Left 192 SCA crimp GrB VDE",39,"Unisub HD 4U Left 192 ports, 192 SC/APC simplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-4L-4822-PBVD","Unisub HD 4U Left 192 LCA crimp GrB VDE",39,"Unisub HD 4U Left 192 ports, 96 LC/APC duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
["UHD-4L-48B3-PBVD","Unisub HD 4U Left 192 LCAsh crimp GB VDE",40,"Unisub HD 4U Left 192 ports, 96 LC/APC shuttered duplex adapters, with Pigtails, Grade B, VDE Germany Colour Coding, with Crimp splice trays"]
[]
["Without Pigtails"]
["ADPT =","Adapters only, no splice capability"]
["UHD-1L-486C-ADPT","Unisub HD 1U Left 48 SCsx adpt, green",37,"Unisub HD 1U Left 48 ports, 48 SC/APC simplex adapters, Adapters only, no splice capability"]
["UHD-1L-726C-ADPT","Unisub HD 1U Left 72 SCsx adpt, green",37,"Unisub HD 1U Left 72 ports, 72 SC/APC simplex adapters, Adapters only, no splice capability"]
["UHD-1L-7222-ADPT","Unisub HD 1U Left 36 LCdx adpt, green",37,"Unisub HD 1U Left 36 ports, 18 LC/APC duplex adapters, Adapters only, no splice capability"]
["UHD-1L-96B3-ADPT","Unisub HD 1U Left 48 LCdx shut adpt grn",39,"Unisub HD 1U Left 48 ports, 24 LC/APC shuttered duplex adapters, Adapters only, no splice capability"]
["UHD-2L-486C-ADPT","Unisub HD 2U Left 96 SCsx adpt, green",37,"Unisub HD 2U Left 96 ports, 96 SC/APC simplex adapters, Adapters only, no splice capability"]
["UHD-2L-726C-ADPT","Unisub HD 2U Left 144 SCsx adpt, green",38,"Unisub HD 2U Left 144 ports, 144 SC/APC simplex adapters, Adapters only, no splice capability"]
["UHD-2L-7222-ADPT","Unisub HD 2U Left 72 LCdx adpt, green",37,"Unisub HD 2U Left 72 ports, 36 LC/APC duplex adapters, Adapters only, no splice capability"]
["UHD-2L-96B3-ADPT","Unisub HD 2U Left 96 LCdx shut adpt grn",39,"Unisub HD 2U Left 96 ports, 48 LC/APC shuttered duplex adapters, Adapters only, no splice capability"]
["UHD-3L-486C-ADPT","Unisub HD 3U Left 144 SCsx adpt, green",38,"Unisub HD 3U Left 144 ports, 144 SC/APC simplex adapters, Adapters only, no splice capability"]
["UHD-3L-726C-ADPT","Unisub HD 3U Left 216 SCsx adpt, green",38,"Unisub HD 3U Left 216 ports, 216 SC/APC simplex adapters, Adapters only, no splice capability"]
["UHD-3L-7222-ADPT","Unisub HD 3U Left 108 LCdx adpt, green",38,"Unisub HD 3U Left 108 ports, 54 LC/APC duplex adapters, Adapters only, no splice capability"]
["UHD-3L-96B3-ADPT","Unisub HD 3U Left 144 LCdx shut adpt grn",40,"Unisub HD 3U Left 144 ports, 72 LC/APC shuttered duplex adapters, Adapters only, no splice capability"]
["UHD-4L-486C-ADPT","Unisub HD 4U Left 192 SCsx adpt, green",38,"Unisub HD 4U Left 192 ports, 192 SC/APC simplex adapters, Adapters only, no splice capability"]
["UHD-4L-726C-ADPT","Unisub HD 4U Left 288 SCsx adpt, green",38,"Unisub HD 4U Left 288 ports, 288 SC/APC simplex adapters, Adapters only, no splice capability"]
["UHD-4L-7222-ADPT","Unisub HD 4U Left 144 LCdx adpt, green",38,"Unisub HD 4U Left 144 ports, 72 LC/APC duplex adapters, Adapters only, no splice capability"]
["UHD-4L-96B3-ADPT","Unisub HD 4U Left 192 LCdx shut adpt grn",40,"Unisub HD 4U Left 192 ports, 96 LC/APC shuttered duplex adapters, Adapters only, no splice capability"]